**Layout instructions for 31-0006 (Moondance)**

Schematic: 33-0006

Assembly: 30-0006

Artwork/Raw PCB: 31-0006

CAD files (PADs): 34-0006

Pallet drawing (if applicable): 32-0006

General board requirements:

PCB material and thickness: 0.062” thick; FR-4; 1-ounce CU clad; ENIG

Rough shape: 160mm X 120mm

Layers: 4

Layer designations:

1: Top components and routes

2: Plane (GND\_SIGNAL)

3: Plane (VCC)

4: Bottom components and routes

Component placement and routining:

* See the DXF file